NOOTA USER MANUAL

This is a description of the function of all of the various circuits that make up the NOOTA board. The basic modules on the board consist of a MidiToCV converter, Glide, two VCOs, a Noise source, a Voltage controlled State Variable Filter, a Mixer for the signal sources, a Mixer for the filter outputs, nine control voltage processors, two envelope generators and a low frequency oscillator.